{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910133884303321"]
[null,null,"Titolo",null,"IEEE standard for low-rate wireless networks . Amendment 1 Physical layer utilizing China medical bands"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 2016"]
[null,null,"ISBN",null,"1-5044-0780-6"]
[null,null,"Descrizione fisica",null,"1 online resource (27 pages)"]
[null,null,"Disciplina",null,"621.384"]
[null,null,"Soggetti",null,"Wireless communication systems - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,null,"Sommario/riassunto","The Ministry of Industry and Information Technology (MIIT) of the Peoples Republic of China has approved the 174-216 MHz, 407-425 MHz, and 608-630 MHz bands for medical information transmission. China medical band (CMB) devices operating within these bands conform to a set of rules specified in MIIT Doc 423-2005, which restricts use of the band to only medical, non-voice use under direction of a healthcare practitioner, among other requirements. A physical layer (PHY) for devices operating on Chinese approved bands for medical signals is defined in this amendment."]