{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910135291603321"]
[null,null,"Titolo",null,"IEEE standard test specifications for varistor surge-protective devices"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 1982"]
[null,null,"ISBN",null,"0-7381-0924-X"]
[null,null,"Descrizione fisica",null,"1 online resource (16 pages)"]
[null,null,"Disciplina",null,"621.381"]
[null,null,"Soggetti",null,"Electronic apparatus and appliances - Thermal properties"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Varistors for surge-protective applications on systems with dc to 420 Hz frequency and voltages equal to or less than 1000 V rms, or 1200 V dc, are covered. Definitions, service conditions, and a series of test criteria for determining the electrical characteristics of the varistors are provided. The tests are intended as design tests and provide a means of comparing various surge-protective devices."]