{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910135430603321"]
[null,null,"Titolo",null,"IEEE Std 1101.3-1993 : IEEE Mechanical Standard for Conduction-Cooled and Air-Cooled 10 Su Modules / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 1993"]
[null,null,"ISBN",null,"0-7381-2757-4"]
[null,null,"Descrizione fisica",null,"1 online resource (iv, 27 pages) : illustrations"]
[null,null,"Disciplina",null,"620.00286"]
[null,null,"Soggetti",null,"Environmental engineering"]
[{"$nulls":4},"Reliability (Engineering)"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Withdrawn Standard. Withdrawn Date: Jan 15, 2001. No longer endorsed by the IEEE. The mechanical design requirements for conduction-cooled and air-cooled modules of the 10SU by 6.375 in (161.9 mm) format are established. The specification of dimensions and tolerances is intended to ensure the mechanical intermateability of modules within associated subracks. The basic dimension, frames, PWBs, materials, assembly, and chassis interface of single-sided and double-sided modules are covered."]