{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910135515603321"]
[null,null,"Titolo",null,"IEEE Std 299.1-2013 / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : IEEE, , 2014"]
[null,null,"ISBN",null,"0-7381-8895-6"]
[null,null,"Descrizione fisica",null,"1 online resource (96 pages)"]
[null,null,"Disciplina",null,"621.38224"]
[null,null,"Soggetti",null,"Shielding (Electricity)"]
[{"$nulls":4},"Shielding (Radiation)"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This standard provides uniform measurement procedures for determining the shielding effectiveness of electromagnetic (EM) shielding for a variety of enclosures and boxes having all dimensions between 0.1 m and 2 m in the radio frequency range not addressed by IEEE Std 299(TM)-2006. This standard is divided into two parts: Part I - 0.75 m to 2 m and Part II - physically small (<; 0.75 m) but electrically large enclosures. In addition to a number of annexes aiding the measurement of shielding effectiveness of these enclosures, Annex I addresses physically small and electrically small enclosures, and Annex J addresses electrically small enclosures in reverberation chambers. Problems occurring in the testing of small enclosures having linear dimension less than 2 m are very different from determining the shielding effectiveness of large rooms and broad depending on the actual size of the enclosure itself. A number of other annexes are included that address rationale, mathematical formulas, selection of measurement techniques, preliminary measurement and repairs, wall-mounted monopoles, impedance mismatch correction, and using isolated monopoles in outer reverberation chambers."]