{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910135520303321"]
[null,null,"Titolo",null,"IEEE standard for rectangular metallic waveguides and their interfaces for frequencies of 110 GHz and above . Part 1 Frequency bands and waveguide dimensions"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 2013"]
[null,null,"ISBN",null,"0-7381-8086-6"]
[null,null,"Descrizione fisica",null,"1 online resource (12 pages)"]
[null,null,"Disciplina",null,"621.381331"]
[null,null,"Soggetti",null,"Dielectric wave guides"]
[{"$nulls":4},"Wave guides - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Specifications for the waveguide (including aperture dimensions, frequency range, cutoff frequency, etc.) are given in this standard. This standard considers the tolerances of the waveguide aperture dimensions and the effect these have on the electrical properties (in terms of return loss, transmission loss, etc.) of the waveguide."]