{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910135989403321"]
[null,null,"Titolo",null,"IEEE Guide for Selection and Design of Aluminum Sheaths for Power Cables / / Institute of Electrical and Electronics Engineers (IEEE)"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : Institute of Electrical and Electronics Engineers (IEEE), , 1989"]
[null,null,"ISBN",null,"0-7381-0797-2"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Disciplina",null,"669.722"]
[null,null,"Soggetti",null,"Aluminum"]
[{"$nulls":4},"Cables"]
[{"$nulls":4},"Design - Methodology"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","The purpose of this guide is as follows: to outline requirements and establish design guidelines for the selection of aluminum sheaths for extra-high, high-, medium-, and low-voltage cables; to establish basic installation parameters for aluminum-sheathed cables; to provide references to industry standards and codes incorporating design and installation requirements of aluminum-sheathed cables; to provide a comprehensive bibliography of literature related to the subject. This guide covers power cables incorporating aluminum sheaths, except those of the SF/sub 6/ rigid-bus type."]