{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910136434603321"]
[null,null,"Titolo",null,"ANSI/IEEE Std 430-1976 : IEEE Standard Procedures for the Measurement of Radio Noise from Overhead Power Lines / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York, N.Y. : , : IEEE, , 1976"]
[null,null,"ISBN",null,"1-5044-0344-4"]
[null,null,"Descrizione fisica",null,"1 online resource (14 pages) : illustrations"]
[null,null,"Disciplina",null,"620.23"]
[null,null,"Soggetti",null,"Noise - Measurement"]
[{"$nulls":4},"Electric lines"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","The purpose of this standard is to establish uniform procedures for the measurement of radiation of radio noise from overhead power lines with meters that conform to American National Standards. A uniform procedure is a prerequisite to comparisons of radio-noise performance of various overhead power lines. The procedure applies in the frequency range of 0.015 to 30 MHz. A procedure for measurements in the frequency range of 20 to 1000 MHz, which is to be used only as a guide, is also presented."]