{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910136446403321"]
[null,null,"Titolo",null,"IEEE Std 345-1972 (ANSI C57.100-1974) : IEEE standard test procedure for thermal evaluation of oil-immersed distribution transformers / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway, New Jersey : , : IEEE, , 1972"]
[null,null,"ISBN",null,"1-5044-0310-X"]
[null,null,"Descrizione fisica",null,"1 online resource (10 pages)"]
[null,null,"Disciplina",null,"621.310420287"]
[null,null,"Soggetti",null,"Electric transformers - Testing"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This test procedure is intended to give a direct evaluation of the composite insulation system of an oil-immersed distribution transformer, tested as an integral unit. It is to be noted that the oil in which the transformer is immersed is to be considered a part of the insulation system. It is the intent of the procedure to provide that each component of the insulation structure operate during the test under conditions which are, as nearly as possible, the same as those that it would encounter in service. Thus, it is intended that each component be evaluated in accordance with its actual function."]