{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910136535503321"]
[null,null,"Titolo",null,"AIEE No 700-1953 : AIEE Standard for Aircraft Direct- Current Apparatus Voltage Ratings / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : IEEE, , 1953"]
[null,null,"ISBN",null,"1-5044-0423-8"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Disciplina",null,"629.13252"]
[null,null,"Soggetti",null,"Aerospace engineering"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","It has been widely recognized that there is a distinct need for preferred voltage ratings for aircraft direct-current electric apparatus which will be generally acceptable to manufacturers and users to serve as a basis for voltage standards for aircraft systems and equipment. Many difficulties and much confusion will be eliminated by adopting suitable standard voltage ratings for all aircraft electric equipment. These standard voltages should then be made a part of specifications and nameplates marked accordingly. Apparatus should be designed for satisfactory operation over the voltage ranges given in the table, but with performance not necessarily the same as guaranteed at rated voltage. Performance data and acceptance tests should be on the basis of standard voltages. It is recognized that special applications may require operation over other voltage ranges than those shown as standard."]