{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910137370303321"]
[null,null,"Titolo",null,"IEEE/ANSI Std 24-1984 (Revision of 24-1977) : IEEE Standard Performance Characteristics and Dimensions for Outdoor Apparatus Bushings / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway, New Jersey : , : IEEE, , 1984"]
[null,null,"ISBN",null,"1-5044-0218-9"]
[null,null,"Descrizione fisica",null,"1 online resource (18 pages)"]
[null,null,"Disciplina",null,"621.310420289"]
[null,null,"Soggetti",null,"Electric apparatus and appliances - Safety measures"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This standard covers electrical, dimensional, and related requirements for outdoor power class apparatus bushings which have basic impulse insulation levels of 110 kV and higher. It provides specific values for dimensional and related requirements which are to be interpreted, measured, or tested in accordance with ANSI/IEEE Std 21-1976. Bushings covered by this standard are intended for use as components of oil-filled transformers, oil-filled reactors, and oil circuit breakers."]