{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[4,2,4,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[22,2,22,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910138862203321"]
[null,null,"Titolo",null,"Control of non-conventional synchronous motors / / edited by Jean-Paul Louis"]
[null,null,"Pubbl/distr/stampa",null,"London, : ISTE"]
[{"$nulls":4},"Hoboken, N.J., : Wiley, 2012"]
[null,null,"ISBN",null,"9781118603208"]
[{"$nulls":4},"1118603206"]
[{"$nulls":4},"9781118603192"]
[{"$nulls":4},"1118603192"]
[{"$nulls":4},"9781118603130"]
[{"$nulls":4},"1118603133"]
[{"$nulls":4},"9781299187832"]
[{"$nulls":4},"1299187838"]
[null,null,"Edizione",null,"[1st ed.]"]
[null,null,"Descrizione fisica",null,"1 online resource (440 p.)"]
[null,null,"Collana",null,"ISTE"]
[null,null,"Disciplina",null,"621.46"]
[null,null,"Soggetti",null,"Electric motors, Synchronous - Automatic control"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"Cover; Control of Non-conventional Synchronous Motors; Title Page; Copyright Page; Table of Contents; Introduction; Chapter 1. Self-controlled Synchronous Motor: Principles of Function and Simplified Control Model; 1.1. Introduction; 1.2. Design aspects specific to the self-controlled synchronous machine; 1.3. Simplified model for the study of steady state operation; 1.4. Study of steady-state operation; 1.5. Operation at nominal speed, voltage and current; 1.6. Operation with a torque smaller than the nominal torque; 1.7. Operation with a speed below the nominal speed"]
[{"$nulls":4},"1.8. Running as a generator 1.9. Equivalence of a machine with a commutator and brushes; 1.10. Equations inferred from the theory of circuits with sliding contacts; 1.11. Evaluation of alternating currents circulating in steady state in the damper windings; 1.12. Transposition of the study to the case of a negative rotational speed; 1.13. Variant of the base assembly; 1.14. Conclusion; 1.15. List of the main symbols used; 1.16. Bibliography; Chapter 2. Self-controlled Synchronous Motor: Dynamic Model Including the Behavior of Damper Windings and "]
[{"$nulls":4},"Commutation Overlap; 2.1. Introduction"]
[{"$nulls":4},"2.2. Choice of the expression of Nk 2.3. Expression of fluxes; 2.4. General properties of coefficients ,  and ; 2.5. Electrical dynamic equations; 2.6. Expression of electromechanical variables; 2.7. Expression of torque; 2.8. Writing of equations in terms of co-energy; 2.9. Application to control; 2.10. Conclusion; 2.11. Appendix 1: value of coefficients ,  and ; 2.12. Appendix 2: derivatives of coefficients ,  and ; 2.13. Appendix 3: simplifications for small μ; 2.14. Appendix 4: List of the main symbols used in Chapters 1 and 2; 2.15. Bibliography"]
[{"$nulls":4},"Chapter 3. Synchronous Machines in Degraded Mode 3.1. General introduction; 3.1.1. Analysis of failures of the set converter-machine: converters with MOSFET transistors; 3.2. Analysis of the main causes of failure; 3.2.1. Failure of the inverter; 3.2.2. Other failures; 3.3. Reliability of a permanent magnet synchronous motors drive; 3.3.1. Environmental conditions in the motor industry; 3.3.2. The two reliability reports: MIL-HdbK-217 and RDF2000; 3.3.3. Failure rate of permanent magnet synchronous motors actuators; 3.4. Conclusion"]
[{"$nulls":4},"3.5. Optimal supplies of permanent magnet synchronous machines in the presence of faults 3.5.1. Introduction: the problem of a-b-c controls; 3.6. Supplies of faulty synchronous machines with non-sinusoidal back electromagnetic force; 3.6.1. Generalization of the modeling; 3.6.2. A heuristic approach to the solution; 3.6.3. First optimization of ohmic losses without constraint on the homopolar current; 3.6.4. Second optimization of ohmic losses with the sum of currents of non-faulty phases being zero; 3.6.5. Third optimization of ohmic losses with a homopolar current of zero (in all phases)"]
[{"$nulls":4},"3.6.6. Global formulations"]
[null,null,null,"Sommario/riassunto","Classical synchronous motors are the most effective device to drive industrial production systems and robots with precision and rapidity. However, numerous applications require efficient controls in non-conventional situations.Firstly, this is the case with synchronous motors supplied by thyristor line-commutated inverters, or with synchronous motors with faults on one or several phases.Secondly, many drive systems use non-conventional motors such as polyphase (more than three phases) synchronous motors, synchronous motors with double excitation, permanent magnet linear synchron"]