{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910139603603321"]
[null,null,"Titolo",null,"Conference Record of 2011 Annual IEEE Pulp and Paper Industry Technical Conference"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified], : IEEE, 2011"]
[null,null,"ISBN",null,"9781612842714"]
[{"$nulls":4},"1612842712"]
[null,null,"Descrizione fisica",null,"1 online resource : illustrations"]
[null,null,"Disciplina",null,"676"]
[null,null,"Soggetti",null,"Paper industry"]
[{"$nulls":4},"Papermaking"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Bibliographic Level Mode of Issuance: Monograph"]
[null,null,null,"Sommario/riassunto","A 'condensate load' (condensate in % of a totally full cylinder) over 1% accumulated inside the dryer cylinders of a paper machine is likely to produce a drive overload, eventually increasing the acceleration time or even producing an overload trip. This paper proposes and evaluates a confident online condensate estimation algorithm that gives updated information at preset speeds and when the transition to the rimming stage is detected. The experimental evaluation performed on a 500 mm diameter cylinder, with condensate load between 0.5% up to 25%, confirmed the ability of the algorithm to give accurate estimations within 0.5% intervals of condensate loads. The developed algorithm is a useful tool for the operators, allowing them to take the appropriate decisions according to the severity of the condensate accumulation detected."]