{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910147054303321"]
[null,null,"Titolo",null,"ANSI/IEEE C37.24-1986 (Revision of ANSI/IEEE C37.24-1971) / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified] : , : IEEE, , 1986"]
[null,null,"ISBN",null,"0780310604"]
[{"$nulls":4},"0-7381-1060-4"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Disciplina",null,"551.5271"]
[null,null,"Soggetti",null,"Solar radiation"]
[{"$nulls":4},"Daylight"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Superseded by C37.24-2003. This IEEE Standards product is part of the C37 family on Switchgear, Substations and Protective Relays. This standard applies to all forms of outdoor metal-enclosed switchgear. It covers operating limitations; the effect of ambient temperature, solar radiation, and wind on internal operating temperatures; ventilation and condensation control; enclosure color and finish considerations; current-carrying capabilities of switchgear, and suggested modifications of standard designs."]