{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910147060803321"]
[null,null,"Titolo",null,"IEEE Standard for Boot"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified], : IEEE, 1994"]
[null,null,"ISBN",null,"0-7381-1194-5"]
[null,null,"Descrizione fisica",null,"1 online resource (vi, 262 pages) : illustrations"]
[null,null,"Disciplina",null,"004"]
[null,null,"Soggetti",null,"Computer firmware"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Bibliographic Level Mode of Issuance: Monograph"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,null,"Sommario/riassunto","Firmware is the read-only-memory (ROM)-based software that controls a computer between the time it is turned on and the time the primary operating system takes control of the machine. Open Firmware provides the following: a mechanism for loading and executing programs (such as operating systems) from disks, tapes, network interfaces, and other devices; an ISA-independent method for identifying devices \"plugged in\" to expansion buses and for providing firmware and diagnostics drivers for these devices; an extensible and programmable command language based on the Forth programming language; methods for managing user-configurable options stored in nonvolatile memory; a \"call back\" interface allowing other programs to make use of Open Firmware services; and debugging tools for hardware, firmware, firmware drivers, and system software."]