{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910147239803321"]
[null,null,"Titolo",null,"American national standard for transformers : 230 kV and below 833/958 through 8333/10 417 kVA, single-phase, and 750/862 through 60 000/80 000/100 000 kVA, three-phase without load tap changing ; and 3750/4687 through 60 000/80 000/100 000 kVA with load tap changing-- safety requirements / / Institute of Electrical and Electronics Engineers, American National Standards Institute"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : Institute of Electrical and Electronics Engineers, , 1997"]
[{"$nulls":4},"©2003"]
[null,null,"Descrizione fisica",null,"1 online resource (32 pages)"]
[null,null,"Disciplina",null,"621.314"]
[null,null,"Soggetti",null,"Electric transformers - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Includes index."]
[null,null,null,"Sommario/riassunto","This IEEE Standards product is part of the C57 Family on Power Distribution and Regulating Transformers."]