{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[11,2,11,3],[12,2,12,3],[16,2,16,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910154726203321"]
[null,null,"Titolo",null,"Labyrinth and piano key weirs : PKW 2011 / / editors, Sebastien Erpicum. [et al.]"]
[null,null,"Pubbl/distr/stampa",null,"London : , : Taylor & Francis Group, , 2011"]
[null,null,"ISBN",null,"1-136-63800-8"]
[{"$nulls":4},"0-429-21281-X"]
[{"$nulls":4},"0-203-80406-6"]
[null,null,"Edizione",null,"[1st ed.]"]
[null,null,"Descrizione fisica",null,"1 online resource (314 pages) : illustrations"]
[null,null,"Disciplina",null,"627.883"]
[null,null,"Soggetti",null,"Weirs"]
[{"$nulls":4},"Dams - Design and construction"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Bibliographic Level Mode of Issuance: Monograph"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"Keynote lectures -- Physical modeling : hydraulic capacity -- Physical modeling : downstream fittings -- Numerical modeling -- Hydraulic design -- Planned and existing projects -- Nomenclature, data base, future developments."]
[null,null,null,"Sommario/riassunto","Labyrinth spillways are almost as old as dam engineering. In spite of the fact that they appear as a very good technical-economical compromise, only 0.1% of large dams are equipped with such weirs. The main reason for this is that traditional labyrinth weirs usually cannot be installed on top of concrete gravity dams as they require a large foundat"]