{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[10,2,10,3],[11,2,11,3],[15,2,15,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910164281703321"]
[null,null,"Autore",null,"Sara M. N"]
[null,null,"Titolo",null,"Evaluation and Remediation of Low Permeability and Dual Porosity Environments"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified], : American Society for Testing & Materials, 2002"]
[null,null,"ISBN",null,"0-8031-5463-1"]
[null,null,"Descrizione fisica",null,"1 online resource (190 pages) : illustrations, maps"]
[null,null,"Collana",null,"ASTM special technical publication ; ; 1415"]
[null,null,"Disciplina",null,"628.5/5"]
[null,null,"Soggetti",null,"Soil remediation"]
[{"$nulls":4},"Soil permeability"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Bibliographic Level Mode of Issuance: Monograph"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,"Nota di contenuto",null,"Comparison between various Field and Laboratory Measurements of the Hydraulic Conductivity of three Clay Liners / D Cazaux, G Didier -- Hydraulic Conductivity of a Fractured Aquitard / T Abichou, CH Benson, M Friend, X Wang -- Water Potential Response in Fractured Basalt from Infiltration Events / JM Hubbell, ED Mattson, JB Sisson, DL McElroy -- On The Measurement Of The Hydraulic Properties Of The Environmental Medium / SS Gordji, L Pirouzian -- Pressure-Pulse Test for Field Hydraulic Conductivity of Soils: Is the Common Interpretation Method Adequate? / RP Chapuis, D Cazaux -- Determining the Hydraulic Properties of Saturated, Low-Permeability Geological Materials in the Laboratory: Advances in Theory and Practice / M Zhang, M Takahashi, RH Morin, H Endo, T Esaki -- Evaluation of Constant Head Infiltration Test Analysis Methods for Field Estimation of Saturated Hydraulic Conductivity of Compacted Clay Liners / D Cazaux -- Impact of Residual NAPL on Water Flow and Heavy Metal Transfer in a Multimodal Grain Size Soil under Saturation Conditions: Implications for Contaminant Mobility / R Galvez-Cloutier, J-S Dubé -- Electrokinetic Removal of Phenanthrene from Kaolin Using Different Surfactants and Cosolvents / KR Reddy, RE Saichek -- Transfer of Heavy Metals in a Soil Amended with Geotextiles / L Lassabatere, T Winiarski, RG Cloutier -- Application of the Colloidal Borescope to Determine a Complex Groundwater Flow Pattern / SM Narbutovskih, JP McDonald, R Schalla, MD Sweeney."]