{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":36,"n_cols":5,"rows_kept":36,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[11,2,11,3],[11,4,11,5],[12,2,12,3],[12,4,12,5],[13,2,13,3],[13,4,13,5],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[29,2,29,3],[30,2,30,3],[33,2,33,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA990001736310403321"]
[null,null,"Autore",null,"Hartig, Robert"]
[null,null,"Titolo",null,"Die zersetzungserscheinungen des holzes der nadelholzbaume und der eiche in forstlicher botanischer und chemischer richtung / Robert Hartig"]
[null,null,"Pubbl/distr/stampa",null,"Berlin : J. Springer, 1878"]
[null,null,"Descrizione fisica",null,"151 p. : 21 tav. ; 29 cm"]
[null,null,"Disciplina",null,"676"]
[null,null,"Locazione",null,"FAGBC"]
[null,null,"Collocazione",null,"60 676 A 2"]
[null,null,"Lingua di pubblicazione",null,"Italiano"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,"2.","Record Nr.",null,"UNINA9910254140703321"]
[null,null,"Autore",null,"Low It-Meng"]
[null,null,"Titolo",null,"High Performance Natural Fiber-Nanoclay Reinforced Cement Nanocomposites / / by It-Meng Low, Ahmad Hakamy, Faiz Shaikh"]
[null,null,"Pubbl/distr/stampa",null,"Cham : , : Springer International Publishing : , : Imprint : Springer, , 2017"]
[null,null,"ISBN",null,"3-319-56588-5"]
[null,null,"Edizione",null,"[1st ed. 2017.]"]
[null,null,"Descrizione fisica",null,"1 online resource (VII, 94 p. 45 illus.)"]
[null,null,"Collana",null,"Biobased Polymers, , 2510-3407"]
[null,null,"Disciplina",null,"624.1833"]
[null,null,"Soggetti",null,"Polymers"]
[{"$nulls":4},"Ceramics"]
[{"$nulls":4},"Glass"]
[{"$nulls":4},"Composite materials"]
[{"$nulls":4},"Building materials"]
[{"$nulls":4},"Nanotechnology"]
[{"$nulls":4},"Polymer Sciences"]
[{"$nulls":4},"Ceramics, Glass, Composites, Natural Materials"]
[{"$nulls":4},"Building Materials"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references at the end of each chapters."]
[null,null,"Nota di contenuto",null,"Chemical Compositions and Structure of Natural Fibres -- Natural Fibre Surface Modification by Alkaline treatment -- Nanotechnology and Cement Nanocomposites -- Cement Nanoclay Nanocomposites -- Cement Calcined Nanoclay Nanocomposites."]
[null,null,null,"Sommario/riassunto","This brief describes a novel approach to overcome the disadvantages of hemp fibres in cementitious composites. The authors describe how the new approach includes the combination of thermal pre-treatment of nanoclay (producing calcined nanoclay) and chemical pre-treatment of fibre surfaces to improve the microstructure, mechanical, physical and thermal properties and also durability of hemp fibre reinforced cement composites. In this work, the synthesis of several materials are studied: nanoclay-cement nanocomposite, calcined nanoclay-cement nanocomposite, untreated & treated hemp fabric-reinforced cement composite, hemp fabric-reinforced nanoclay-cement nanocomposite and treated hemp fabric-reinforced nanoclay-cement nanocomposite. The influence of nanoclay on properties of cement paste and hemp "]
[{"$nulls":4},"fabric-reinforced cement composite is also presented together with the influence of NaOH pre-treatment of fibre surfaces on properties of hemp fabric-reinforced cement composite. The authors have aimed this brief at those working on environmental-friendly, biodegradable, building materials."]