{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910258756103321"]
[null,null,"Titolo",null,"IEEE Std 802.15.8-2017 : IEEE Standard for Wireless Medium Access Control (MAC) and Physical Layer (PHY) Specifications for Peer Aware Communications (PAC) / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , [2018]"]
[null,null,"ISBN",null,"1-5044-4612-7"]
[null,null,"Descrizione fisica",null,"1 online resource (322 pages)"]
[null,null,"Disciplina",null,"005.44"]
[null,null,"Soggetti",null,"Distributed operating systems (Computers)"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Physical layer (PHY) and medium access control (MAC) mechanisms are defined in this standard for wireless personal area networks (WPANs) peer aware communications (PAC) optimized for peer-to-peer and infrastructure-less communications with fully distributed coordination. PAC features include discovery for peer information without association, discovery signaling rate typically greater than 100 kb/s, discovery of the number of devices in the network, scalable data transmission rates typically up to 10 Mb/s, group communications with simultaneous membership in multiple groups typically up to 10, relative positioning, security, and operation in selected globally available unlicensed/licensed bands below 11 GHz capable of supporting these requirements."]