{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910263756203321"]
[null,null,"Titolo",null,"ISO/IEC/IEEE 8802-3:2017/Amd. 2:2017(E) : ISO/IEC/IEEE International Standard - Part 3: Standard for Ethernet - Amendment 2: Media Access Control Parameters, Physical Layers, and Management Parameters for 25 Gb/s Operation / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , [2018]"]
[null,null,"ISBN",null,"1-5044-4731-X"]
[null,null,"Descrizione fisica",null,"1 online resource (248 pages)"]
[null,null,"Disciplina",null,"004.68"]
[null,null,"Soggetti",null,"Ethernet (Local area network system)"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This amendment to IEEE Std 802.3-2015 adds Physical Layer (PHY) specifications and management parameters for 25 Gb/s operation over twinaxial copper cabling (25GBASE-CR and 25GBASE-CR-S), electrical backplanes (25GBASE-KR and 25GBASE-KR-S), and multimode fiber (25GBASE-SR). This amendment also specifies a 25 Gigabit Attachment Unit Interface (25GAUI) and optional Energy Efficient Ethernet (EEE)."]