{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[10,2,10,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910296451603321"]
[null,null,"Titolo",null,"IEEE Std C37.30.4-2018 : IEEE Standard for Test Code for Switching and Fault Making Tests for High-Voltage Interrupter Switches, Interrupters or Interrupting Aids Used on or Attached to Switches Rated for Alternating Currents Above 1000 V / / Switchgear of the IEEE Power and Energy Society"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 2018"]
[null,null,"ISBN",null,"1-5044-5221-6"]
[null,null,"Descrizione fisica",null,"1 online resource (33 pages)"]
[null,null,"Collana",null,"IEEE Std ; ; C37.30.4-2018"]
[null,null,"Disciplina",null,"621.317"]
[null,null,"Soggetti",null,"Electric switchgear - Testing"]
[{"$nulls":4},"Voltage regulators"]
[{"$nulls":4},"High voltages - Testing"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Test code for switching (except capacitive current) and fault making tests for switching devices for alternating current, rated above 1000 V and used indoors, outdoors, or in enclosures is specified in this standard."]