{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":33,"n_cols":5,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3],[16,2,16,3],[16,4,16,5],[17,2,17,3],[17,4,17,5],[18,2,18,3],[18,4,18,5],[19,2,19,3],[20,2,20,3],[24,2,24,3],[25,2,25,3],[28,2,28,3],[29,2,29,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910697884703321"]
[null,null,"Autore",null,"Powell R. W"]
[null,null,"Titolo",null,"Thermal conductivity of selected materials [[electronic resource]] / R. W. Powell, C. Y. Ho, and P. E. Liley"]
[null,null,"Pubbl/distr/stampa",null,"Washington, D.C. : , : U.S. Dept. of Commerce, National Bureau of Standards : , : For sale by the Supt. of Docs., U.S. G.P.O., , [1966]"]
[null,null,"Descrizione fisica",null,"175 unnumbered pages ; ; 29 cm"]
[null,null,"Collana",null,"NSRDS-NBS ; ; 8"]
[null,null,"Soggetti",null,"Thermal conductivity"]
[{"$nulls":4},"Materials - Thermal properties"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Title from title screen (viewed on May 19, 2009)."]
[{"$nulls":4},"\"Issued November 25, 1966.\""]
[{"$nulls":4},"\"Category 5: thermodynamic and transport properties.\""]
[{"$nulls":4},"Digital reproduction; no longer available for sale by the Supt. of Docs."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,"2.","Record Nr.",null,"UNINA9910317676703321"]
[null,null,"Autore",null,"Vicente Antonio T"]
[null,null,"Titolo",null,"Nanostructured Solar Cells"]
[null,null,"Pubbl/distr/stampa",null,"InTechOpen, 2017"]
[null,null,"ISBN",null,"9789535141105"]
[{"$nulls":4},"9535141104"]
[{"$nulls":4},"9789535129363"]
[{"$nulls":4},"9535129368"]
[null,null,"Descrizione fisica",null,"1 online resource (34)"]
[null,null,"Soggetti",null,"The arts"]
[{"$nulls":4},"Writing systems, alphabets"]
[{"$nulls":4},"Computational linguistics"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","The employment of printing techniques as cost-effective methods to fabricate low cost,\nflexible, disposable and sustainable solar cells is intimately dependent on the substrate\nproperties and the adequate electronic devices to be powered by them. Among such\ndevices, there is currently a growing interest in the development of user-oriented and\nmultipurpose systems for intelligent packaging or on-site medical diagnostics, which\nwould greatly benefit from printable solar cells as their energy source for autonomous\noperation.\nThis chapter first describes and analyzes different types of cellulose-based substrates for\nflexible and cost effective optoelectronic and bio devices to be powered by printed solar\ncells. Cellulose is one of the most promising platforms for green recyclable electronics\nand it is fully compatible with large-scale printing techniques, although "]
[{"$nulls":4},"some critical\nrequirements must be addressed. Paper substrates exist in many forms. From common\noffice paper, to packaging cardboard used in the food industry, or nanoscale engineered\ncellulose (e.g. bacterial cellulose). However, it is the structure and content of paper that\ndetermines its end use. Secondly, proof-of-concept of optoelectronic and bio devices produced\nby inkjet printing are described and show the usefulness of solar cells as a power\nsource or as a chemical reaction initiator for sensors."]