{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[11,2,11,3],[12,2,12,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910389743103321"]
[null,null,"Titolo",null,"8802-1AR-2020 - ISO/IEC/IEEE International Standard for Telecommunications and exchange between information technology systems . Part 1AR, Secure device identity : Requirements for local and metropolitan area networks / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York. : , : IEEE, , 2020"]
[null,null,"ISBN",null,"1-5044-6588-1"]
[null,null,"Descrizione fisica",null,"1 online resource (76 pages)"]
[null,null,"Disciplina",null,"341.35"]
[null,null,"Soggetti",null,"Authentication"]
[{"$nulls":4},"Telecommunication - Standards"]
[{"$nulls":4},"Information technology - Standards"]
[{"$nulls":4},"Local area networks (Computer networks) - Standards"]
[{"$nulls":4},"Metropolitan area networks (Computer networks) - Standards"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","A Secure Device Identifier (DevID) is cryptographically bound to a device and supports authentication of the device's identity. An Initial Device Identifier (IDevID) provided by the supplier of a device can be supplemented by Local Device Identifiers (LDevIDs) facilitating enrollment (provisioning of authentication and authorization credentials) by local network administrators."]