{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":34,"n_cols":5,"rows_kept":34,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3],[14,2,14,3],[14,4,14,5],[15,2,15,3],[15,4,15,5],[16,2,16,3],[16,4,16,5],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,2,21,3],[22,2,22,3],[23,2,23,3],[26,2,26,3],[27,2,27,3],[31,2,31,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910702830803321"]
[null,null,"Autore",null,"Roche Christine M"]
[null,null,"Titolo",null,"High-solids enzymatic saccharification screening method for lignocellulosic biomass [[electronic resource] /] / Christine M. Roche and Jonathan J. Stickel"]
[null,null,"Pubbl/distr/stampa",null,"[Golden, Colo.] : , : National Renewable Energy Laboratory, , [2009?]"]
[null,null,"Descrizione fisica",null,"1 online resource (1 unnumbered page) : illustrations"]
[null,null,"Collana",null,"NREL/PO ; ; 510-45751"]
[null,null,"Soggetti",null,"Biomass conversion - Research"]
[{"$nulls":4},"Ethanol as fuel - Research"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Title from title screen (viewed on November 6, 2009)."]
[{"$nulls":4},"\"31st Symposium on Biotechnology for Fuels and Chemicals, May 2-6, 2009 in San Francisco, CA.\""]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,"2.","Record Nr.",null,"UNINA9910437762903321"]
[null,null,"Autore",null,"Tejchman Jacek"]
[null,null,"Titolo",null,"Continuous and discontinuous modelling of fracture in concrete using FEM / / Jacek Tejchman and Jerzy Bobiski"]
[null,null,"Pubbl/distr/stampa",null,"Berlin ; ; New York, : Springer, 2012, c2013"]
[null,null,"ISBN",null,"3-642-28463-9"]
[null,null,"Edizione",null,"[1st ed.]"]
[null,null,"Descrizione fisica",null,"1 online resource (416 p.)"]
[null,null,"Collana",null,"Springer series in geomechanics and geoengineering, , 1866-8763"]
[null,null,"Disciplina",null,"624.15136"]
[null,null,"Soggetti",null,"Concrete construction - Mathematical models"]
[{"$nulls":4},"Structural analysis (Engineering) - Mathematical models"]
[{"$nulls":4},"Finite element method"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,"Nota di contenuto",null,"Introduction -- General -- Literature Overview -- Theoretical Models -- Discrete Lattice Model -- Epilogue."]
[null,null,null,"Sommario/riassunto","The book analyzes a quasi-static fracture process in concrete and reinforced concrete by means of constitutive models formulated within continuum mechanics. A continuous and discontinuous modelling approach was used. Using a continuous approach, numerical analyses were performed using a finite element method and three different enhanced continuum models: isotropic elasto-plastic, isotropic damage and anisotropic smeared crack one. The models were equipped with a characteristic length of micro-structure by means of a non-local and a second-gradient theory. So they could properly describe the formation of localized zones with a certain thickness and spacing and a related deterministic size effect. Using a discontinuous FE approach, numerical results of cracks using a cohesive crack model and XFEM were presented which were also properly regularized. Finite element analyses were performed with concrete elements under monotonic uniaxial compression, uniaxial tension, bending and shear-extension. Concrete beams under cyclic loading were also simulated using a coupled elasto-plastic-damage approach. Numerical simulations were performed at macro- and meso-level of concrete. A stochastic and deterministic size effect was carefully investigated. In the case of reinforced concrete specimens, FE calculations were carried out with bars, slender and short beams, columns, corbels and tanks. Tensile and shear failure mechanisms were studied. Numerical results were "]
[{"$nulls":4},"compared with results from corresponding own and known in the scientific literature laboratory and full-scale tests.    ."]