{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[11,2,11,3],[12,2,12,3],[16,2,16,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910437786103321"]
[null,null,"Titolo",null,"TOF range-imaging cameras / / Fabio Remondino, David Stoppa, editors"]
[null,null,"Pubbl/distr/stampa",null,"Berlin ; ; New York, : Springer, 2013"]
[null,null,"ISBN",null,"3-642-27523-0"]
[null,null,"Edizione",null,"[1st ed. 2013.]"]
[null,null,"Descrizione fisica",null,"1 online resource (243 p.)"]
[null,null,"Disciplina",null,"681.25"]
[null,null,"Soggetti",null,"Image processing - Digital techniques"]
[{"$nulls":4},"Electronic surveillance"]
[{"$nulls":4},"Three-dimensional imaging"]
[{"$nulls":4},"Time-of-flight mass spectrometry"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,"Nota di contenuto",null,"State-of-the-art of ToF Range Image Sensors and their applications -- SPAD-based Sensors -- Electronic-based Sensors -- Sensors based on in-pixel Photo-mixing devices -- Understanding and ameliorating mixed pixels and multipath interference in AMCW LiDAR -- 3D Cameras: errors, calibration and orientation.- ToF cameras for architectural survey -- Indoor navigation using range imaging.-ToF cameras and stereo systems: comparison and data fusion -- ToF cameras in ambient-assisted living applications -- Application overview of commercial ToF cameras."]
[null,null,null,"Sommario/riassunto","Today the cost of solid-state two-dimensional imagers has dramatically dropped, introducing low cost systems on the market suitable for a variety of applications, including both industrial and consumer products. However, these systems can capture only a two-dimensional projection (2D), or intensity map, of the scene under observation, losing a variable of paramount importance, i.e., the arrival time of the impinging photons. Time-Of-Flight (TOF) Range-Imaging (TOF) is an emerging sensor technology able to deliver, at the same time, depth and intensity maps of the scene under observation. Featuring different sensor resolutions, RIM cameras serve a wide community with a lot of applications like monitoring, architecture, life sciences, robotics, etc. This book will bring together experts from the sensor and metrology side in order to collect the state-of-art researchers in these fields working with RIM cameras. All the aspects in "]
[{"$nulls":4},"the acquisition and processing chain will be addressed, from recent updates concerning the photo-detectors, to the analysis of the calibration techniques, giving also a perspective onto new applications domains."]