{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[10,2,10,3],[11,2,11,3],[15,2,15,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910454661303321"]
[null,null,"Titolo",null,"Slope stability in surface mining [[electronic resource] /] / edited by William A. Hustrulid, Michael K. McCarter, Dirk J.A. Van Zyl"]
[null,null,"Pubbl/distr/stampa",null,"Littleton, Colo., : Society for Mining, Metallurgy, and Exploration, 2001"]
[null,null,"ISBN",null,"1-5231-3822-X"]
[{"$nulls":4},"0-87335-295-5"]
[null,null,"Descrizione fisica",null,"1 online resource (461 p.)"]
[null,null,"Disciplina",null,"622/.292"]
[null,null,"Soggetti",null,"Strip mining"]
[{"$nulls":4},"Slopes (Soil mechanics)"]
[{"$nulls":4},"Electronic books."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"section 1. Rock slope design considerations -- section 2. Case studies in rock slope stability -- section 3. Stability of wawste rock embankments -- section 4. Tailings and heap leaching."]
[null,null,null,"Sommario/riassunto","As we enter the 21st century, mines are being planned to reach depths of more than 1,100 meters, waste rock embankments have surpassed 600 meters in height, tailings dams have reached heights of 200 meters, and heap leach facilities have topped 150 meters. The push toward higher, deeper, and steeper, along with the larger and more productive equipment in use today, continues to test our tools and capabilities. Slope Stability in Surface Mining documents the progressive rise in technical understanding and sophistication in the field. Only by continuously collecting and exchanging information ca"]