{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[10,2,10,3],[11,2,11,3],[15,2,15,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910463084303321"]
[null,null,"Autore",null,"Ayan Cosan"]
[null,null,"Titolo",null,"Formation testing [[electronic resource] ] : fluid analysis / / Cosan Ayan"]
[null,null,"Pubbl/distr/stampa",null,"Richardson, TX, : Society of Petroleum Engineers, c2012"]
[null,null,"ISBN",null,"1-61399-167-3"]
[null,null,"Descrizione fisica",null,"1 online resource (230 p.)"]
[null,null,"Collana",null,"Getting up to speed"]
[null,null,"Soggetti",null,"Reservoir oil pressure"]
[{"$nulls":4},"Fluid dynamics"]
[{"$nulls":4},"Electronic books."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,"Nota di contenuto",null,"\"\"Foreword\"\"; \"\"Contents\"\"; \"\"Compositional Modeling of Oil-Based Mud-Filtrate Cleanup During Wireline Formation Tester Sampling\"\"; \"\"Reservoir Fluid Identification and Testing With a Modular Formation Tester in an Aging Field\"\"; \"\"Applications of Real-Time Downhole pH Measurements\"\"; \"\"Downhole Measurement of Methane Content and GOR in Formation Fluid Samples\"\"; \"\"New Downhole Fluid Analyzer Tool for Improved Reservoir Characterization\"\"; \"\"Integration of Geochemical, Mud-Gas, and Downhole-Fluid Analyses for the Assessment of Compositional Grading-Case Studies\"\""]
[{"$nulls":4},"\"\"Real Time Integration of Reservoir Modeling and Formation Testing\"\"\"\"Determination of Producible Hydrocarbon Type and Oil Quality in Wells Drilled with Synthetic Oil-Based Muds\"\"; \"\"Novel Technology Provides Cost Effective Answers for Revival of a Mature Oilfield\"\"; \"\"Real-Time Determination of Filtrate Contamination During Openhole Wireline Sampling by Optical Spectroscopy\"\"; \"\"Identification of Vertical Compartmentalization and Compositional Variation by Downhole Fluid Analysis;  Towards a Continuous Downhole Fluid Log\"\""]
[{"$nulls":4},"\"\"Asphaltene Gravitational Gradient in a Deepwater Reservoir as Determined by Downhole Fluid Analysis\"\"\"\"In-Situ Density and Viscosity Measured by Wireline Formation Testers\"\"; \"\"Focused Sampling of Reservoir Fluids Achieves Undetectable Levels of Contamination\"\"; \"\"Assessing Reservoir Connectivity Through Biomarker and Bulk Compositional Gradient Analysis\"\"; \"\"In-Situ Optical Fluid Analysis as an Aid to Wireline Formation Sampling\"\"; \"\"EOS-Based Downhole Fluid Characterization\"\""]
[{"$nulls":4},"\"\"Investigation of Formation Connectivity Using Asphaltene Gradient Log Predictions Coupled with Downhole Fluid Analysis\"\"\"\"Interpretation of DFA Color Gradients in Oil Columns Using the Flory-Huggins Solubility Model\"\""]