{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910520209103321"]
[null,null,"Titolo",null,"1562-2021 - IEEE Recommended Practice for Sizing Stand-Alone Photovoltaic (PV) Systems - Redline / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York, USA : , : IEEE, , 2021"]
[null,null,"ISBN",null,"1-5044-8378-2"]
[null,null,"Descrizione fisica",null,"1 online resource (61 pages)"]
[null,null,"Disciplina",null,"621.31"]
[null,null,"Soggetti",null,"Electric power"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Provided in this recommended practice is information to assist in sizing the array and battery of a stand-alone photovoltaic (PV) system. Systems considered in this recommended practice consist of PV as the only power source and a battery for energy storage. These systems also commonly employ controls to protect the battery from being over- or under-charged and may employ a power conversion subsystem (inverter or converter). This recommended practice is applicable to all stand-alone PV systems where PV is the only charging source. This recommended practice does not include PV hybrid systems nor grid-connected systems. This recommended practice covers lead-acid batteries only; nickel-cadmium and other battery types are not included. This recommended practice does not include the sizing of the system controller, inverter, wiring, or other system components."]