{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[6,2,6,3],[7,2,7,3],[12,2,12,3],[12,4,12,5],[13,2,13,3],[13,4,13,5],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910697919503321"]
[null,null,"Titolo",null,"Niger, rapport mensuel sur la sécurité alimentaire [[electronic resource]]"]
[null,null,"Pubbl/distr/stampa",null,"[Washington, D.C.], : [FEWS NET]"]
[null,null,"Descrizione fisica",null,"volumes : digital, PDF file"]
[null,null,"Soggetti",null,"Food supply - Niger"]
[{"$nulls":4},"Famines - Niger"]
[null,null,"Lingua di pubblicazione",null,"Francese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Periodico"]
[null,null,null,"Note generali","Issues have distinctive titles on web site."]
[{"$nulls":4},"Description based on Aout 2005; title from title screen (viewed on Jan. 23, 2009)."]
[{"$nulls":4},"Final issue consulted."]
[null,"2.","Record Nr.",null,"UNINA9910135336803321"]
[null,null,"Titolo",null,"High-voltage switchgear and controlgear . Part 111 Automatic circuit reclosers and fault interrupters for alternating current systems up to 38 kV / / International Electrotechnical Commission, Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , [2012]"]
[null,null,"ISBN",null,"0-7381-7309-6"]
[null,null,"Descrizione fisica",null,"1 online resource (129 pages) : illustrations"]
[null,null,"Disciplina",null,"621.46"]
[null,null,"Soggetti",null,"Electric controllers"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This part of IEC 62271 applies to all overhead, pad mounted, dry vault and submersible single or multi-pole alternating current automatic circuit reclosers and fault interrupters for rated maximum voltages above 1 000 V and up to 38 kV. Devices that require a dependent manual operation are not covered by this standard. In order to simplify this standard where possible, the term recloser/FI (reclosers/FIs) has been substituted for automatic circuit recloser or fault interrupter or both."]