{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[14,2,14,3],[15,2,15,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910699506003321"]
[null,null,"Autore",null,"Parker Bradford H"]
[null,null,"Titolo",null,"A comparison of the capability of sensitivity level 3 and sensitivity level 4 fluorescent penetrants to detect fatigue cracks in aluminum [[electronic resource] /] / Bradford H. Parker"]
[null,null,"Pubbl/distr/stampa",null,"Greenbelt, Md. : , : National Aeronautics and Space Administration, Goddard Space Flight Center, , [2009]"]
[null,null,"Descrizione fisica",null,"1 online resource (16 pages) : illustrations"]
[null,null,"Collana",null,"NASA/TM ; ; 2009-215850"]
[null,null,"Soggetti",null,"Inspection"]
[{"$nulls":4},"Quality control"]
[{"$nulls":4},"Nondestructive tests"]
[{"$nulls":4},"Cracks"]
[{"$nulls":4},"Penetrants"]
[{"$nulls":4},"Probability theory"]
[{"$nulls":4},"Metal fatigue"]
[{"$nulls":4},"Detection"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Title from title screen (viewed on Oct. 22, 2010)."]
[{"$nulls":4},"\"December 2009.\""]
[null,null,null,"Nota di bibliografia","Includes bibliographical references (page 16)."]