{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910699717403321"]
[null,null,"Titolo",null,"Surface infiltration rates of permeable surfaces [[electronic resource] ] : six month update (November 2009 through April 2010) / / by Michael Borst ... [and others]"]
[null,null,"Pubbl/distr/stampa",null,"Edison, N.J. : , : National Risk Management Research Laboratory, Water Supply and Water Resources Division, U.S. Environmental Protection Agency, , [2010]"]
[null,null,"Descrizione fisica",null,"1 online resource (28 pages) : illustrations (some color)"]
[null,null,"Soggetti",null,"Seepage"]
[{"$nulls":4},"Permeability"]
[{"$nulls":4},"Runoff - Management - Technological innovations"]
[{"$nulls":4},"Parking lots - Environmental aspects - Technological innovations"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","\"June 2010.\""]
[{"$nulls":4},"\"EPA/600/R-10/083.\""]
[{"$nulls":4},"Title from title screen (viewed Aug. 27, 2010)."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references (page 28)."]