{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[12,2,12,3],[13,2,13,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910701331903321"]
[null,null,"Titolo",null,"Caution : foundry at work"]
[null,null,"Pubbl/distr/stampa",null,"[Atlanta, Ga.] : , : NIOSH, National Institute for Occupational Safety and Health, , [1997]"]
[null,null,"Soggetti",null,"Dust - Removal"]
[{"$nulls":4},"Ventilation"]
[{"$nulls":4},"Foundries - Dust control"]
[{"$nulls":4},"Hazardous substances - Safety measures"]
[{"$nulls":4},"Foundry workers - Health and hygiene"]
[{"$nulls":4},"Occupational diseases - Prevention"]
[{"$nulls":4},"Industrial hygiene"]
[{"$nulls":4},"Educational films."]
[{"$nulls":4},"Documentary films."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Videoregistrazione"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Streaming videos available as RM files (10 min., 17 sec., sd., col.) available in low (56 kbps) and high (300 kbps) resolutions."]
[{"$nulls":4},"Title from title frame."]
[{"$nulls":4},"\"NIOSH, National Institute for Occupational Safety and Health\"--opening credits frame."]
[{"$nulls":4},"\"1997\"--Video home page."]
[{"$nulls":4},"\"Audience: Foundry safety engineers and managers\"--Video home page."]
[{"$nulls":4},"\"NIOSH Pub. #98-109d\"--Video home page."]
[null,null,null,"Sommario/riassunto","Describes how foundry workers can be protected from hazards such as silica dust, fumes, heat and noise through engineering controls such as ventilation and isolation."]