{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910703596003321"]
[null,null,"Autore",null,"Prahl Duncan"]
[null,null,"Titolo",null,"Moisture risk in unvented attics due to air leakage paths / / prepared by D. Prahl and M. Shaffer"]
[null,null,"Pubbl/distr/stampa",null,"Golden, CO : , : U.S. Department of Energy, Energy Efficiency & Renewable Energy, , [2014]"]
[null,null,"Descrizione fisica",null,"1 online resource (ix, 27 pages) : illustrations (some color)"]
[null,null,"Soggetti",null,"Attics - Moisture - Testing"]
[{"$nulls":4},"Buildings - Airtightness"]
[{"$nulls":4},"Dampness in buildings"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Title from title screen (viewed on Sept. 14, 2015)."]
[{"$nulls":4},"\"Prepared for the National Renewable Energy Laboratory on behalf of the U.S. Department of Energy's Building America Program, Office of Energy Efficiency and Renewable Energy.\""]
[{"$nulls":4},"\"November 2014.\""]
[{"$nulls":4},"\"DOE/GO-102014-4526.\""]
[null,null,null,"Nota di bibliografia","Includes bibliographical references (pages 26-27)."]