{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910705300703321"]
[null,null,"Autore",null,"Girsang I. P."]
[null,null,"Titolo",null,"Gearbox and drivetrain models to study dynamic effects of modern wind turbines : preprint / / I.P. Girsang [and four others]"]
[null,null,"Pubbl/distr/stampa",null,"[Golden, Colo.] : , : National Renewable Energy Laboratory, , October 2013"]
[null,null,"Descrizione fisica",null,"1 online resource (9 pages) : color illustrations"]
[null,null,"Collana",null,"NREL/CP ; ; 5500-58960"]
[null,null,"Soggetti",null,"Wind turbines - Design and construction - Computer simulation"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Published through SciTech Connect."]
[{"$nulls":4},"\"Presented at the IEEE Energy Conversion Congress and Exposition, September 15-19, 2013, Denver, Colorado.\""]
[{"$nulls":4},"\"October 2013.\""]
[null,null,null,"Nota di bibliografia","Includes bibliographical references (pages 8-9)."]
[null,null,null,"Sommario/riassunto","Wind turbine drivetrains consist of components that directly convert kinetic energy from the wind to electrical energy. Guaranteeing robust and reliable drivetrain designs is therefore important to minimize turbine downtime. Current drivetrain models often lack the ability to model both the impacts of electrical transients as well as wind turbulence and shear in one package. In this work, the capability of the FAST wind turbine computer-aided engineering tool, developed by the National Renewable Energy Laboratory, is enhanced through integration of a dynamic model of the drivetrain. The dynamic drivetrain model is built using Simscape in the MATLAB/Simulink environment and incorporates detailed electrical generator models. This model can be used in the future to test advanced control schemes to extend life of the gearbox."]