{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910707866403321"]
[null,null,"Titolo",null,"2D/3D Program work summary report / / edited by P.S. Damerell, J. W. Simons"]
[null,null,"Pubbl/distr/stampa",null,"Washington, DC : , : Office of Nuclear Regulatory Research, U.S. Nuclear Regulatory Commission, , June 1993"]
[null,null,"Descrizione fisica",null,"1 online resource (various pagings) : illustrations"]
[null,null,"Collana",null,"GRS ; ; 100"]
[{"$nulls":4},"International agreement report ; ; 0126"]
[null,null,"Soggetti",null,"Pressurized water reactors - Loss of coolant"]
[{"$nulls":4},"Pressurized water reactors - Safety measures"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","\"MPR-1345.\""]
[{"$nulls":4},"\"Prepared jointly by Japan Atomic Energy Institute, Gesellschaft fuer Anlagen-und Reaktorsicherheit, Siemens AG, UB KWU, U.S. Nuclear Regulatory Commission, Los Alamos National Laboratory, MPR Associates, Inc.\""]
[{"$nulls":4},"\"June 1993.\""]
[{"$nulls":4},"\"Prepared as part of arrangement on Research Participation and Technical Exchange between the federal minister for research and technology of the Federal Republic of Germany (BMFT) and the Japan Atomic Energy Research Institute (JAERI) and the United States Nuclear Regulatory Commission (USNRC) in a coordinated analytical and experimental study of the thermo-hydraulic behavior of emergency core coolant during the refill and reflood phase of a loss-of-coolant accident in a pressurized water reactor (the 2D/3D Program).\""]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]