{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[4,2,4,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[13,2,13,3],[14,2,14,3],[17,2,17,3],[24,2,24,3],[24,4,24,5],[25,2,25,3],[25,4,25,5],[26,2,26,3],[28,2,28,3],[29,2,29,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910460539003321"]
[null,null,"Titolo",null,"Hot working guide : a compendium of processing maps / / edited by Y.V.R.K. Prasad, K.P. Rao, S. Sasidhara"]
[null,null,"Pubbl/distr/stampa",null,"Materials Park, OH : , : ASM International, , [2015]"]
[{"$nulls":4},"©2015"]
[null,null,"ISBN",null,"1-62708-092-9"]
[{"$nulls":4},"0-87170-598-2"]
[{"$nulls":4},"1-68015-949-6"]
[null,null,"Edizione",null,"[Second edition.]"]
[null,null,"Descrizione fisica",null,"1 online resource (638 p.)"]
[null,null,"Soggetti",null,"Metals - Hot working"]
[{"$nulls":4},"Alloys - Mechanical properties"]
[{"$nulls":4},"Metals - Formability"]
[{"$nulls":4},"Electronic books."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,"Nota di contenuto",null,"05445G_Front Matter_rev; Blank Page; Combined; Ch1; P 1-3 corrected 2; P 4-8 corrected 2; P 9-13 corrected 3; P 14-16 corrected; P 17-20 corrected 2; P 21-25 corrected; P 26-30 corrected; Ch 2; 2 AL INTRODUCTION corrected; 2.1 Al 99.999 % purity; 2.2 Al 99.99; 2.3 Al 99.9%; 2.4 Al 99.5%; 2.5 Al-0.1Mg; 2.6 Al-0.5Mg; 2.7 Al-1Mg; 2.8 Al-2Mg; 2.9 Al-5Mg; 2.10 Al-Fe; 2.11 Al-Fe-Mn; 2.12 Al-10Zn; 2.13 Al 1235 corrected; 2.14 2024 Al alloy; 2.15 Al 2099; 2.16 2124 Al Alloy (PM) corrected 2; 2.17 2519+Ag; 2.18 2618 Al; 2.19 Al-5.9Cu-.0.5Mg; 2.20 Al-5.9Cu-0.5Mg-0.06Sn; 2.21 Al 3003; 2.22 Al 4043"]
[{"$nulls":4},"2.23 Al 55562.24 6061 Al; 2.25 Al 6063; 2.26 6201 Al; 2.27 Al 6351; 2.28 6951 Al; 2.29 7020 Al corrected; 2.30 7075 Al; 2.31 7075 Al + 4 Mn; 2.32 7085 Al alloy; 2.33 8090 Al; 2.34 8090 Al low Li; 2.35 8090 Al + Be corrected; 2.36 Al-4Li alloy; 2.37 Al-3.2Cu-1.6Li; 2.38 Al-B4C composite; 2.39 1100Al-10 SiC; 2.40 2124 5 SiC corrected; 2.41 2124 10 SiCp; 2.42 Al 2124-15 SiC VHP; 2.43 2124+15 % SiC Extr; 2.44 2124+20 % SiC; 2.45 2024 Al +20 SiCw; 2.46 2014 20 Al2O3; 2.47 2124+30 % SiC; 2.48 Al-TiC in situ composite; 2.49 6061 Al+11 SiC; 2.50 6061 Al 18 SiC; 2.51 6061+20 SiC; 2.52 6061 10 Al2O3"]
[{"$nulls":4},"2.53 7075-8CfiberCh3; 3 CU INTRODUCTION corrected; 3.1 OFHC Cu 2ppm; 3.2 OFHC copper 11 ppm; 3.3 OFHC 30 ppm; 3.4 OFHC 40 ppm; "]
[{"$nulls":4},"3.5 ETP copper 100 ppm; 3.6 ETP copper 180 ppm; 3.7 ETP copper 220  ppm; 3.8 ETP copper 260  ppm; 3.9 ETP copper PM corrected; 3.10 cu3zn; 3.11 cu10zn; 3.12 Cu-15Zn; 3.13 cu21zn; 3.14 cu23zn; 3.15 cu28zn; 3.16 cu30zn; 3.17 cu42zn; 3.18 cu44zn; 3.19 cu47zn; 3.20 cu51zn; 3.21 Cu25Zn12Ni; 3.22 Cu30Zn0.2Zr; 3.23 Cu40Zn3Pb; 3.24 Cu42Zn12Ni; 3.25 cup0.5al; 3.26 cu2al corrected; 3.27 cu4al; 3.28 cu6al; 3.29 Cu-30Ni; 3.30 Cu-6Ni1Si corrected; Ch4; 4 FE INTRODUCTION"]
[{"$nulls":4},"4.1 Alpha Iron 4.2 Gamma Iron; 4.3 Fe-5Ni; 4.4 Fe-0.5Co; 4.5 Fe-5Co; 4.6 Fe-5Mo; 4.7 Fe-5Si; 4.8 Mild Steel; 4.9 Microalloyed steel; 4.10 Maraging steel; 4.11 CRNO steel; 4.12 CRGO steel; 4.13 Ledeburitic steel; 4.14 Kanthal K5 corrected; 4.15 304 stainless steel; 4.16 304L stainless steel; 4.17 316 stainless steel commercial; 4.18 316L stainless steel; 4.19 316 LN stainless; 4.20 15Cr-15Ni-2Mo steel; 4.21 15Cr-15Ni-2Mo-0.2Ti corrected; 4.22 15Cr-15Ni-2Mo-0.3Ti; 4.23 15Cr-15Ni-2Mo-0.4Ti corrected; 4.24 SUS303 free cutting steel; 4.25 18Mn18Cr0.5N stainless steel corrected"]
[{"$nulls":4},"4.26 12Ni-14Co-3Cr-1Mo stainless steel 4.27 3Cr20Ni10W2 Aus SS corrected 2; 4.28 IN028 superalloy; 4.29 9Cr-1Mo Ferritic Steel; 4.30 9Cr-1Mo-0.5Nb Stabilized steel corrected; 4.31 630 Maraging steel; 4.32 13Cr-0.2C  Martensitic SS; 4.33 1Cr11Ni2W2Mo steel corrected 2; 4.34 22Cr1Ni0.7NbN Duplex ss; 4.35 Fe-24Ni-11Cr-1Mo-3Ti corrected; 4.36 FeAl WA corrected; 4.37 FeAl GA corrected; 4.38 Fe3Al alloy; 4.39 Fe3Al Binary alloy; 4.40 Fe3Al Ti alloy; 4.41 Fe3Al Mn alloy; 4.42 Fe3Al Cr alloy; Ch5; 5 MG INTRODUCTION corrected; 5.1 Magnesium; 5.2 Mg-Nano Alumina; 5.3 Mg-3Al alloy corrected"]
[{"$nulls":4},"5.4 AZ31 AC CH"]
[null,"2.","Record Nr.",null,"UNINA9910712224503321"]
[null,null,"Titolo",null,"Pacific Northwest National Laboratory investigation of stress corrosion cracking in nickel-base alloys : behavior of alloy 152 and 52 welds"]
[null,null,"Pubbl/distr/stampa",null,"United States Nuclear Regulatory Commission, Office of Nuclear Regulatory Research"]
[{"$nulls":4},"Washington, D.C"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]