{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910713449703321"]
[null,null,"Titolo",null,"Octane requirements of 1975 model year automobiles fueled with unleaded gasoline"]
[null,null,"Pubbl/distr/stampa",null,"[Ann Arbor, Mich.] : , : Technology Assessment and Evaluation Branch, Emission Control Technology Division, Office of Mobile Source Air Pollution Control, Environmental Protection Agency, , August 1975"]
[null,null,"Descrizione fisica",null,"1 online resource (approximately 27 pages) : illustrations"]
[null,null,"Soggetti",null,"Gasoline - Anti-knock and anti-knock mixtures - Standards"]
[{"$nulls":4},"Gasoline - Anti-knock and anti-knock mixtures - Testing"]
[{"$nulls":4},"Automobiles - Fuel consumption - Measurement"]
[{"$nulls":4},"Technical reports."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","\"August 1975.\""]
[{"$nulls":4},"\"75-28 JLB.\""]
[{"$nulls":4},"Report number assigned by the National Service Center for Environmental Publications (NSCEP); TAEB7528JLB."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references (page 21)."]