{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910713485303321"]
[null,null,"Autore",null,"Beverage Joseph P."]
[null,null,"Titolo",null,"Comparison of flume and towing methods for verifying the calibration of a suspended-sediment sampler / / by Joseph P. Beverage and James C. Futrell, II"]
[null,null,"Pubbl/distr/stampa",null,"Minneapolis, Minnesota : , : U.S. Geological Survey, , 1986"]
[null,null,"Descrizione fisica",null,"1 online resource (v, 12 pages) : illustrations"]
[null,null,"Collana",null,"Water-resources investigations report ; ; 86-4193"]
[null,null,"Soggetti",null,"Water - Sampling - Equipment and supplies - Calibration"]
[{"$nulls":4},"Suspended sediments"]
[{"$nulls":4},"Flumes - Calibration"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Also available online in PDF format from the U.S. Geological Survey Warehouse (http://pubs.er.usgs.gov/)."]
[{"$nulls":4},"\"Prepared in cooperation with the U.S. Agricultural Research Service, U.S. Bureau of Reclamation, U.S. Forest Service, U.S. Bureau of Land Management, and the U.S. Federal Highways Administration.\""]
[null,null,null,"Nota di bibliografia","Includes bibliographical references (page 12)."]