{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[10,2,10,3],[11,2,11,3],[15,2,15,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910786506103321"]
[null,null,"Autore",null,"Kim Youngkyoo"]
[null,null,"Titolo",null,"Advances in organic light-emitting devices / / Youngkyoo Kim and Chang-Sik Ha"]
[null,null,"Pubbl/distr/stampa",null,"[Stafa-Zuerich] : , : Trans Tech Publications, , [2008]"]
[null,null,"ISBN",null,"3-03813-244-6"]
[null,null,"Descrizione fisica",null,"1 online resource (153 p.)"]
[null,null,"Collana",null,"Materials science foundations, , 1422-3597 ; ; volume 40"]
[null,null,"Disciplina",null,"620.11295"]
[null,null,"Soggetti",null,"Organic scintillators"]
[{"$nulls":4},"Electroluminescent devices"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,"Nota di contenuto",null,"Advances in Organic Light-Emitting Device; Preface; Table of Contents; List of Abbreviations; Table of Contents; 1. History of the OLED; 2. Introduction to OLEDs; 2.1 Classification of OLEDs. 2.2 OLED Using Small Organic Molecules; 2.3 PLED Using Emissive Polymers; 2.4 Hybrid OLED; 2.5 Kinds of Devices According to Function and Structure; 3. The Physics behind OLEDs; 3.1 Basic Mechanism; 3.2 Charge Carrier Injection and Transport; 3.3 Delayed EL Owing to Low Charge Carrier Mobility; 3.4 Generation of Singlet and Triplet Excitons in OLEDs; 3.5 Efficiency of OLEDs"]
[{"$nulls":4},"3.6 Exciton Energy Transfer from Donor (Host) to Acceptor (Guest)4. Organic Materials (Small Molecules ) for OLEDs; 4.1 Hole-Injecting Materials; 4.2 Hole-Transporting Materials; 4.3 Light-Emitting Materials (Organic Light-Emitters); 4.4 Hole-Blocking Materials. 4.5 Electron-Transporting Materials; 4.6 Electron-Injecting Materials. 4.7 Electrodes; 5. Polymeric Materials for PLEDs; 5.1 Polymers for Buffer Layer; 5.2 Light-Emitting Polymers; 5.3 Hole-Blocking/Electron-Transporting/Electron-Injecting Polymers. 5.4 Electrode Materials; 6. Materials for Hybrid OLEDs"]
[{"$nulls":4},"6.1 Materials for All-Organic HOLEDs6.2 Materials for Organic-Inorganic HOLEDs; 7. Reliability and Lifetime; 7.1 Moisture Effect; 7.2 Oxygen Effect; 7.3 Impurity Effect; 7.4 Progressive Electrical Short; 7.5 Solvent and Polymer Side-Chain Effects in PLEDs; 7.6 Intrinsic Material Stability and Luminance Decay Mechanism; 8. OLED Displays; 8.1 Passive Matrix-Organic Light-emitting Display (PM-OLED); 8.2 Active-Matrix - Organic Light-Emitting Display (AM-OLED); 8.3 Full-Color OLED Displays; 9. Ongoing Challenges; 9.1 Flexible OLED; 9.2 Organic "]
[{"$nulls":4},"Light-Emitting Transistors"]
[{"$nulls":4},"9.3 OLED for Lighting Applications10. OLED Market Trends and Outlook; 10.1 OLED Market Trends; 10.2 Outlook"]
[null,null,null,"Sommario/riassunto","Organic electroluminescence (OEL) is the phenomenon of electrically-driven emission of light from organic materials; including both fluorescent and phosphorescent organic solids. The organic light-emitting device (OLED), which exploits OEL emission from organic semiconducting thin films (with thicknesses of less than a few hundred nanometers), sandwiched between electrodes, has attracted keen interest in its application to flat-panel displays, due to its high luminous efficiency, low driving voltage, tunable colors as well as a convenient device-structure design and low fabrication costs when"]