{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910795157603321"]
[null,null,"Autore",null,"Steffes-lai Daniela"]
[null,null,"Titolo",null,"Approximation methods for high dimensional simulation results : parameter sensitivity analysis and propagation of variations for process chains / / Daniela Steffes-lai"]
[null,null,"Pubbl/distr/stampa",null,"Berlin : , : Logos Verlag, , [2014]"]
[{"$nulls":4},"©2014"]
[null,null,"ISBN",null,"3-8325-9163-X"]
[null,null,"Descrizione fisica",null,"1 online resource (ix, 219 pages) : illustrations"]
[null,null,"Disciplina",null,"003.5"]
[null,null,"Soggetti",null,"Sensitivity theory (Mathematics) - Simulation methods"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","PublicationDate: 20140630"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references."]
[null,null,null,"Sommario/riassunto","Long description: This work addresses the analysis of a sequential chain of processing steps, which is particularly important for the manufacture of robust product components. In each processing step, the material properties may have changed and distributions of related characteristics, for example, strains, may become inhomogeneous. For this reason, the history of the process including design-parameter uncertainties becomes relevant for subsequent processing steps. Therefore, we have developed a methodology, called PRO-CHAIN, which enables an efficient analysis, quantification, and propagation of uncertainties for complex process chains locally on the entire mesh. This innovative methodology has the objective to improve the overall forecast quality, specifically, in local regions of interest, while minimizing the computational effort of subsequent analysis steps. We have demonstrated the benefits and efficiency of the methodology proposed by means of real applications from the automotive industry."]