{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[10,2,10,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910805667303321"]
[null,null,"Autore",null,"Noe Mathias"]
[null,null,"Titolo",null,"380 kV Superconducting Fault Current Limiter Feasibility Study / / Mathias Noe [and many others]"]
[null,null,"Pubbl/distr/stampa",null,"Karlsruhe : , : KIT Scientific Publishing, , 2023"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Disciplina",null,"621.3815"]
[null,null,"Soggetti",null,"Superconductors - Industrial applications"]
[{"$nulls":4},"Electric power systems - Protection"]
[{"$nulls":4},"Electric power transmission - Economic aspects"]
[{"$nulls":4},"Technical reports."]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,null,"Sommario/riassunto","In this study the technical and economic feasibility of a 380 kV, 5 kA resistive type superconducting fault current limiter was investigated. Conceptual designs were developed with superconducting tapes cooled by liquid nitrogen and arranged in bifilar coils. A cryostat was designed using FEM simulations taking into account the non-linear voltage distribution. For the complete system including current limiting reactors and cooling system, the investment and operation costs were calculated."]