{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[5,2,5,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[17,2,17,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910824558403321"]
[null,null,"Autore",null,"Anjum Bushra"]
[null,null,"Titolo",null,"Bandwidth allocation for video under quality of service constraints / / Bushra Anjum, Harry Perros"]
[null,null,"Pubbl/distr/stampa",null,"London, England ; ; Hoboken, New Jersey : , : ISTE : , : Wiley, , 2015"]
[{"$nulls":4},"©2015"]
[null,null,"ISBN",null,"1-119-07317-0"]
[{"$nulls":4},"1-119-07315-4"]
[{"$nulls":4},"1-119-07316-2"]
[null,null,"Descrizione fisica",null,"1 online resource (153 p.)"]
[null,null,"Collana",null,"FOCUS Networks and Telecommunication Series"]
[null,null,"Disciplina",null,"005.746"]
[null,null,"Soggetti",null,"Data compression (Telecommunication)"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Description based upon print version of record."]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,"Nota di contenuto",null,"Cover; Title Page; Copyright; Contents; Biographies; Bushra Anjum; Harry G. Perros; Acronyms; Introduction; I.1. QoS evolution in the IP network; I.1.1. Real Time Protocol (RTP); I.1.2. Integrated Services (IntServ); I.1.3. Differentiated Services (DiffServ); I.1.4. Multiprotocol Label Switching (MPLS); I.2. Elements of QoS architecture; I.2.1. Traffic classification; I.2.2. Queuing and scheduling policies; I.2.3. Policing of a packet flow; I.2.4. CAC; I.2.5. Traffic engineering; I.3. Problem definition: bandwidth allocation under QoS constraints"]
[{"$nulls":4},"I.3.1. Bandwidth allocation based on the packet loss rate - literature reviewI.3.2. Bandwidth allocation based on end-to-end delay - literature review; I.4. Organization of the book; 1: Partitioning the End-to-End QoS Budget to Domains; 1.1. The need for adding percentiles; 1.2. Calculation of the weight function; 1.2.1. Exponential components with identical rate parameters; 1.2.2. Exponential components with different rate parameters; 1.2.3. Two-stage Coxian; 1.3. Interprovider quality of service; 1.4. Single source shortest path using Dijkstra's algorithm; 1.5. Conclusions"]
[{"$nulls":4},"2: Bandwidth Allocation for Video: MMPP2 Arrivals2.1. The queueing network under study; 2.2. Single-node decomposition; 2.3. Bandwidth estimation based on bounds; 2.4. Validation; 2.5. Conclusions; 3: Bandwidth Allocation for Video: MAP2 Arrivals; 3.1. The queueing network under study; 3.2. End-to-end delay estimation based on bounds; 3.2.1. The interpolation function; 3.3. Validation; 3.4. Video "]
[{"$nulls":4},"traces; 3.5. Conclusions; 4: Bandwidth Allocation for Video: Video Traces; 4.1. The proposed algorithm; 4.2. Test traces; 4.3. Bandwidth requirements for homogeneous flows"]
[{"$nulls":4},"4.4. Bandwidth allocation under percentile delay and jitter constraints4.5. Bandwidth allocation under percentile delay, average jitter and packet loss rate constraints; 4.6. Conclusions; Bibliography; Index"]
[null,null,null,"Sommario/riassunto","We present queueing-based algorithms to calculate the bandwidth required for a video stream so that the three main Quality of Service constraints, i.e., end-to-end delay, jitter and packet loss, are ensured.  Conversational and streaming video-based applications are becoming a major part of the everyday Internet usage. The quality of these applications (QoS), as experienced by the user, depends on three main metrics of the underlying network, namely, end-to-end delay, jitter and packet loss. These metrics are, in turn, directly related to the capacity of the links that the video traffic trave"]