{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[2,4,2,5],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[10,2,10,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910879792403321"]
[null,null,"Autore",null,"Demirdelen Ismet"]
[null,null,"Titolo",null,"Nutzung der keramischen Glühkerze als Sensorelement / / Ismet Demirdelen"]
[null,null,"Pubbl/distr/stampa",null,"Karlsruhe : , : KIT Scientific Publishing, , 2024"]
[null,null,"Descrizione fisica",null,"1 online resource"]
[null,null,"Collana",null,"Forschungsberichte aus der industriellen Informationstechnik; ; 29"]
[null,null,"Disciplina",null,"620.14"]
[null,null,"Soggetti",null,"Detectors - Design and construction"]
[{"$nulls":4},"Interface circuits"]
[{"$nulls":4},"Ceramics"]
[null,null,"Lingua di pubblicazione",null,"Tedesco"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Nota di bibliografia","Includes bibliographical references and index."]
[null,null,null,"Sommario/riassunto","This work presents methods for using the ceramic glow plug as a sensor element. This means that the ceramic glow plug will not only perform its conventional task as a heating element but will also provide information, such as motor speed, from the combustion chamber as a sensor. The main focus will be on the change in resistance, particularly under the influence of a temperature change, in the immediate vicinity of the ceramic glow plug."]