{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3],[12,2,12,3],[12,4,12,5],[13,2,13,3],[13,4,13,5],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[26,2,26,3],[27,2,27,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNINA9910211165803321"]
[null,null,"Titolo",null,"ANSI N42.18-2004 (Reaffirmation of ANSI N42.18-1980; Redesignation of ANSI N13.10-1974) : American national standard, specification and performance of on-site instrumentation for continuously monitoring radioactivity in effluents / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York, New York : , : IEEE, , 1974"]
[null,null,"ISBN",null,"1-5044-5707-2"]
[null,null,"Descrizione fisica",null,"1 online resource (23 pages)"]
[null,null,"Disciplina",null,"363.7063"]
[null,null,"Soggetti",null,"Environmental monitoring"]
[{"$nulls":4},"Radioactive pollution"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This standard provides recommendations for the selection of instrumentation specific to the continuous monitoring and quantification of radioactivity in effluents released to the environment. The effluent streams considered may contain radioactive gases, liquids, particulates, or dissolved solids singly or in combination. This standard specifies detection capabilities, physical and operating limits, reliability, and calibration requirements and sets forth minimum performance requirements for effluent monitoring instrumentation. Unless otherwise specified, the criteria herein refer to the total system. This standard applies only to monitoring during routine operation that includes abnormal releases. Emergency situations, where additional performance capability will be required, are a matter of separate consideration."]
[null,"2.","Record Nr.",null,"UNINA9910891237303321"]
[null,null,"Titolo",null,"American pharmaceutical review"]
[null,null,"Pubbl/distr/stampa",null,"Indianapolis, IN, : Russell Pub"]
[null,null,"ISSN",null,"1938-2669"]
[null,null,"Disciplina",null,"615"]
[null,null,"Soggetti",null,"Pharmaceutical technology - United States"]
[{"$nulls":4},"Pharmaceutical industry - United States"]
[{"$nulls":4},"Drug Industry"]
[{"$nulls":4},"Technology, Pharmaceutical"]
[{"$nulls":4},"Pharmaceutical industry"]
[{"$nulls":4},"Pharmaceutical technology"]
[{"$nulls":4},"Periodical"]
[{"$nulls":4},"Periodicals."]
[{"$nulls":4},"United States"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Periodico"]