{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[12,2,12,3],[13,2,13,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996216256703316"]
[null,null,"Titolo",null,"Material aspects in automotive catalytic converters"]
[null,null,"Pubbl/distr/stampa",null,"[Place of publication not identified], : Deutsche Gesellschaft für Materialkunde, 2002"]
[null,null,"ISBN",null,"1-280-55827-X"]
[{"$nulls":4},"9786610558278"]
[{"$nulls":4},"3-527-60053-1"]
[null,null,"Descrizione fisica",null,"1 online resource (281 pages)"]
[null,null,"Disciplina",null,"629.25/28"]
[null,null,"Soggetti",null,"Automobiles - Materials - Catalytic converters"]
[{"$nulls":4},"Automotive Engineering"]
[{"$nulls":4},"Mechanical Engineering"]
[{"$nulls":4},"Engineering & Applied Sciences"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Note generali","Bibliographic Level Mode of Issuance: Monograph"]
[null,null,null,"Sommario/riassunto","MACC 2001 is the successor meeting of the first international conference on Materials Aspects in Automotive Catalytic Converters, MACC '97, and concentrates on the high-temperature mechanical and oxidation behaviour of both metal-supported and ceramic-supported automotive catalysts. The metal-supported catalyst is based on a ferritic steel with 5-8% aluminium, 17-22% chromium and small additions of reactive elements. More than 20,000,000 units were produced in 1999. The ceramic-supported catalytic converter is based on corderite. The production rate of ceramic-supported catalysts is much higher. Both materials have specific advantages and disadvantages which determine the application for a given car model. In addition to these two basic groups of catalytic carriers, the scope of the conference also refers to coating aspects, since the influence of the coating composition is becoming more and more important. The car and car-supplying industries report on their future requirements with respect to performance and service life. Maintaining good performance is mandatory particularly in the view of thinner supports and higher temperatures. This book examines the area."]