{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996278271803316"]
[null,null,"Titolo",null,"IEEE Std 1596.3-1996 : IEEE Standard for Low-Voltage Differential Signals (LVDS) for Scalable Coherent Interface (SCI) / / Institute of Electrical and Electronics Engineers"]
[null,null,"Pubbl/distr/stampa",null,"New York, N.Y. : , : Institute of Electrical and Electronics Engineers, , 1996"]
[null,null,"ISBN",null,"0-7381-3136-9"]
[null,null,"Descrizione fisica",null,"1 online resource (v, 30 pages)"]
[null,null,"Disciplina",null,"620.00218"]
[null,null,"Soggetti",null,"Standards, Engineering"]
[{"$nulls":4},"Tolerance (Engineering)"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Scalable Coherent Interface (SCI), specified in IEEE Std 1596-1992, provides computer-bus-like services but uses a collection of fast point-to-point links instead of a physical bus in order to reach far higher speeds. The base specification defines differential ECL signals, which provide a high transfer rate (16 bits are transferred every 2 ns), but are inconvenient for some applications. IEEE Std 1596.3-1996, an extension to IEEE Std 1596-1992, defines a lower-voltage differential signal (as low as 250 mV swing) that is compatible with low-voltage CMOS, BiCMOS and GaAs circuitry."]