{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[11,2,11,3],[12,2,12,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279556903316"]
[null,null,"Titolo",null,"ANSI/IEEE Std C62.2-1987 : IEEE Guide for the Application of Gapped Silicon-Carbide Surge Arresters for Alternating Current Systems / / IEEE Power Engineering Society Surge Protective Devices Committee, IEEE Standards Board, American National Standards Institute"]
[null,null,"Pubbl/distr/stampa",null,"Piscataway : , : IEEE, , 1989"]
[null,null,"ISBN",null,"0-7381-3016-8"]
[null,null,"Descrizione fisica",null,"1 online resource (56 pages)"]
[null,null,"Disciplina",null,"621.317"]
[null,null,"Soggetti",null,"Electric apparatus and appliances - Protection"]
[{"$nulls":4},"Transients (Electricity) - Standards"]
[{"$nulls":4},"Electric power system stability - Standards"]
[{"$nulls":4},"Silicon carbide - Electric properties"]
[{"$nulls":4},"Electric currents, Alternating"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","This standard covers the application of gapped silicon-carbide surge arresters to safeguard electric power equipment against the hazards of abnormally high voltage surges of various origins. Such overvoltages may cause flashovers and serious damage to equipment, thereby jeopardizing the supply of power to users. It is essential to prevent this by the proper coordination of surge protection devices with the insulation strength of the protected equipment."]