{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279580603316"]
[null,null,"Titolo",null,"IEEE Standard Specification of General-Purpose Laboratory Cathode-Ray Oscilloscopes / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York, N.Y. : , : IEEE, , 1970"]
[null,null,"ISBN",null,"0-7381-4557-2"]
[null,null,"Descrizione fisica",null,"1 online resource (18 pages)"]
[null,null,"Collana",null,"IEEE Std ; ; No.311"]
[null,null,"Disciplina",null,"621.3"]
[null,null,"Soggetti",null,"Digital oscilloscopes"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","The purposes of this Standard are: to document the minimum information that users of general-purpose laboratory cathode-ray oscilloscopes typically need; to provide potential purchasers and others with a common means for making comparisons between instruments; and to provide uniformity of information from manufacturers. This Standard applies primarily to general-purpose laboratory cathode-ray oscilloscopes; it does not necessarily apply to specific kinds of oscilloscopes, such as those employing sampling techniques, nor to storage oscilloscopes, spectrum analyzers, television monitors, or other instruments using cathode-ray tube displays."]