{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[10,2,10,3],[11,2,11,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279603303316"]
[null,null,"Titolo",null,"ANSI C63.5-2017 (Revision of ANSI C63.5-2005) - Redline : American National Standard for Electromagnetic Compatibility : Radiated Emission Measurements in Electromagnetic Interference (EMI) Control : Calibration and Qualification of Antennas (9 kHz to 40 GH) / / IEEE"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 2017"]
[null,null,"ISBN",null,"1-5044-4853-7"]
[null,null,"Descrizione fisica",null,"1 online resource (215 pages)"]
[null,null,"Collana",null,"ANSI ; ; C63.5-2017"]
[null,null,"Disciplina",null,"621.38224"]
[null,null,"Soggetti",null,"Electromagnetic compatibility"]
[{"$nulls":4},"Electromagnetic interference - Measurement"]
[{"$nulls":4},"Antenna arrays"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","Methods for determining antenna factors of antennas used for radiated emission measurements in electromagnetic interference (EMI) control from 9 kHz to 40 GHz are provided. Antennas included are linearly polarized antennas such as loops, rods (monopoles), tuned dipoles, biconical dipoles, log-periodic dipole arrays, biconical and log-periodic dipole array hybrids, broadband horns, etc., that are used in measurements prescribed by ANSI C63.4 and ANSI C63.10. The antenna calibration methods include standard site method (i.e., three-antenna method), reference antenna method, equivalent capacitance substitution method, standard transmit loop method, standard antenna method, and standard field method."]