{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["report2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"report2","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,5],[1,2,1,3],[1,4,1,5],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[9,2,9,3],[10,2,10,3]],"flags":["formulas_cached_only"]}
[null,"1.","Record Nr.",null,"UNISA996279870403316"]
[null,null,"Titolo",null,"IEEE guide for operation and maintenance of hydro-generators"]
[null,null,"Pubbl/distr/stampa",null,"New York : , : IEEE, , 1974"]
[null,null,"ISBN",null,"0-7381-4216-6"]
[null,null,"Descrizione fisica",null,"1 online resource (64 pages)"]
[null,null,"Disciplina",null,"621.46"]
[null,null,"Soggetti",null,"Electric motors, Synchronous"]
[{"$nulls":4},"Hydraulic turbines"]
[{"$nulls":4},"Standards, Engineering"]
[null,null,"Lingua di pubblicazione",null,"Inglese"]
[null,null,"Formato",null,"Materiale a stampa"]
[null,null,null,"Livello bibliografico","Monografia"]
[null,null,null,"Sommario/riassunto","General recommendations are provided for the operation, loading, and maintenance of hydro-generators and generator/motors (pump/turbines), having salient pole rotors and conventional cooling systems (as distinct from conductor cooling systems). The term hydro-generator refers to a generator driven by a hydraulic turbine or waterwheel. Types of units and bases of rating are included. Generators with cylindrical rotors are not covered."]